Exercise 4:

1. The mode field size: 3 bits
2. The register field size: 6 bits
3. The address field size: 18 bits
4. The opcode field size : 32-(3+6+18) = 5 bits